
***********************************************************************************************
		PON PC Software Installation Instructions

1. Run PON V1.0.15 SETUP.EXE to connect PON.

2. Operating environment Installation
    32-bit system: Install Synchronization.msi in the directory"..\Microsoft Sync Framework\x86\".
    64-bit system: Install Synchronization.msi in the directory"..\Microsoft Sync Framework\x64\".

3. If the PON.exe doesn't work after installed, please run dotNetFx40_Full_x86_x64.exe.

4. Driver Installation
   E series PON : Run EPON Serial Port Driver.EXE, after double-clicking the program,
   then click "°²×°" button.Wait a few seconds prompt "drive pre-installed successfully",
   complete the driver installation.

   A series PON : 
	Windows XP: The first time you connect to the computer system hardware installation 
	wizard pops up,select "Install from a list or specific location",after click next,
	select "Include this location in the search",browse to the installation directory
	"PON Driver" folder,after click next,the system automatically install drivers,tip 
	hardware installation is complete,click "Finish" to complete the driver installation.
	
	Windows 7 : After the device is connected to the computer ,select Start ¡ú Control Panel
	¡úDevice Manager,select "Other Devices" and right click "PON OPM",select "update 
	Driver Software",click "Browse my computer for driver sofeware",browse to the 
	installation directory "PON Driver" folder,after click next,the system automatically 
	install drivers,tip has successfully updated driver software,click "close" to complete 
	the driver installation.

   	Windows 10: 
  	After the device is connected to the computer,Click the Window button,select Settings¡ú
   	Devices¡úConnected devices¡úDevices and printers,select"Other Devices",then right 
   	click"PON OPM",select"Update Driver Software...",click "Search automatically for updated 
   	driver software",the system automatically install drivers,after installation is successful,
   	tip has updated "USB Serial Device",click"close"to complete the driver installation.
************************************************************************************************